Setting up the WAGO e!Display 7300

1. Power up the panel using 24VDC.
2. Panel comes with 2 Ethernet ports, 2 USB and micro SD card slot.
3. Startup program on the Web based management
4. Log in with user name : Admin and password : wago
5. Change the IP address to 192.168.1.1
6. From your PC web browser configure the screen
7. Change password to had
8. From Application –>PLC1 changed to PFC200
9. Add the PFC200 URL : URL//192.168.1.15/webvisu.htm
10. Change the start page to PFC200
11. In the PLC web-based management ensure that in PLC runtime services--> e-runtime🡪 webserver enabled is selected.